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· Analog audio output supports balanced/unbalanced audio output (unbalanced access to "+" and "GND")
· Audio sampling rate supports 44.1kHz, 48kHz and 96kHz (24bit)
· Dante solution supports AES67 RTP audio transmission
· Audio output supports 3-level gain adjustment：+18dBu, 0dBu (default) and -10dBV
· Support DC 12V power supply and POE function (IEEE802.3af Class 0)		




AVIP-DE-DAN

This Dante 2CH Analog Audio Decoder is an audio receiver that utilizes the Dante Ultimo solution. It offers both balanced and unbalanced audio output, along with a 3-level gain adjustment feature. The device receives audio signals from the transmitting end over a Dante network, decodes the signals, and outputs them as analog audio. Additionally, it supports Power over Ethernet (POE) functionality.
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Dante 2CH Analog Audio Decoder with POE


							Dante 2CH Analog Audio/ Decoder with POE
AVIP-DE-DAN 
 

SPECIFICATIONS:

	Technical

	Video Network Bandwidth 
	100M

	Audio Formats
	PCM 2.0 44.1kHz/48kHz/96kHz up to 24bit

	Transmission Distance 
	100m (CAT6/6A)

	Control Method
	Dante Controller

	Connection

	Input
	1x DANTE [RJ45 connector, POE]

	
	1x PWR [2-pin phoenix, 3.81mm]

	Output
	1x AUD [6-pin phoenix, 3.81mm]

	Mechanical

	Housing
	Metal Enclosure

	Color
	Black

	Dimensions
	120mm[W] x 47mm[D] x 26mm[H]

	Weight
	186g

	Power Supply
	DC input: 12V

	
	POE input: IEEE802.3af Class 0

	Power Consumption
	1.32W

	Operation Temperature
	32 - 104oF / 0 - 40oC 

	Storage temperature
	-4 - 140oF / -20 - 60oC 

	Relative Humidity
	20 - 90% RH (no condensation)
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